# Async MQTT client for ESP8266 and ESP32

![Build with PlatformIO](https://github.com/marvinroger/async-mqtt-client/workflows/Build%20with%20Platformio/badge.svg)
![cpplint](https://github.com/marvinroger/async-mqtt-client/workflows/cpplint/badge.svg)

An Arduino for ESP8266 and ESP32 asynchronous [MQTT](http://mqtt.org/) client implementation, built on [me-no-dev/ESPAsyncTCP (ESP8266)](https://github.com/me-no-dev/ESPAsyncTCP) | [me-no-dev/AsyncTCP (ESP32)](https://github.com/me-no-dev/AsyncTCP) .

## Features

* Compliant with the 3.1.1 version of the protocol
* Fully asynchronous
* Subscribe at QoS 0, 1 and 2
* Publish at QoS 0, 1 and 2
* SSL/TLS support
* Available in the [PlatformIO registry](http://platformio.org/lib/show/346/AsyncMqttClient)

## Requirements, installation and usage

The project is documented in the [/docs folder](docs).
